*************************************************
*   Description of the content of the archive   *
*************************************************
- Folder:
	- WtrScrewPathB:			pd2 and inp files for the reference runs (BaseCAv = customer average runs, Meas25 = measure runs)
- File:
	- DEERChillerBatchJuly2017.xlsm: 	Microsoft Excel file used to create the CSV files necessary to run the simulations using the Batch Processing feature of eQUEST

*************
*   Notes   *
*************
- The simulations were run using eQUEST 3.65 build 7174 and DOE-2.2 version 48y.
- The chiller efficiency in the measure runs is higher than the customer average runs.
- CHILLER:ELEC-INPUT-RATIO:
	- CAv: 		0.1976117
	- Meas25:	0.1482088