$LIBRARY-ENTRY AirFoil w Dischrg Dampers FPLR  CURVE-FIT       Fan EIR-FPLR    
$Air Foil with Discharge Dampers
   TYPE             = QUADRATIC
   INPUT-TYPE       = COEFFICIENTS
   OUTPUT-MIN       = 0.68
   OUTPUT-MAX       = 1
   COEFFICIENTS     = ( .227143,  1.178929, -0.410714 )
   ..
$LIBRARY-ENTRY AirFoil w Inlet Vanes FPLR      CURVE-FIT       Fan EIR-FPLR    
$Air Foil with Inlet Vanes
   TYPE             = QUADRATIC
   INPUT-TYPE       = COEFFICIENTS
   OUTPUT-MIN       = 0.48
   OUTPUT-MAX       = 1
   COEFFICIENTS     = ( .584345, -0.579167,  0.970238 )
   ..
$LIBRARY-ENTRY ForCurve w Dischrg Dampers FPLR CURVE-FIT       Fan EIR-FPLR    
$Forward Curved Centrifugal with Discharge Dampers
   TYPE             = QUADRATIC
   INPUT-TYPE       = COEFFICIENTS
   OUTPUT-MIN       = 0.22
   OUTPUT-MAX       = 1
   COEFFICIENTS     = ( .190667,  0.310000,  0.500000 )
   ..
$LIBRARY-ENTRY ForCurve w Inlet Vanes FPLR     CURVE-FIT       Fan EIR-FPLR    
$Forward Curved Centrifugal with Inlet Vanes
   TYPE             = QUADRATIC
   INPUT-TYPE       = COEFFICIENTS
   OUTPUT-MIN       = 0.22
   OUTPUT-MAX       = 1
   COEFFICIENTS     = ( .339619, -0.848139,  1.495671 )
   ..
$LIBRARY-ENTRY Vane Axial w Var Pitch FPLR     CURVE-FIT       Fan EIR-FPLR    
$Vane Axial with Variable Pitch Blades
   TYPE             = QUADRATIC
   INPUT-TYPE       = COEFFICIENTS
   OUTPUT-MIN       = 0.15
   OUTPUT-MAX       = 1
   COEFFICIENTS     = ( .212048, -0.569286,  1.345238 )
   ..
$LIBRARY-ENTRY Variable Speed Drive FPLR       CURVE-FIT       Fan EIR-FPLR    
$Any fan with Variable Speed Drive
   TYPE             = QUADRATIC
   INPUT-TYPE       = COEFFICIENTS
   OUTPUT-MIN       = 0.10
   OUTPUT-MAX       = 1
   COEFFICIENTS     = ( .219762, -0.874784,  1.652597 )
   ..
$LIBRARY-ENTRY DW-Gas-Pilotless-HIR-fPLR       CURVE-FIT       Gas DW-Heater   
  TYPE=QUADRATIC      COEF=( 0, 0.99945700, 0.00054300)
  INPUT-TYPE COEFFICIENTS ..
$LIBRARY-ENTRY Residential Var Vol-Fan EIR     CURVE-FIT       Fan EIR-FPLR    
   TYPE = CUBIC   INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = ( 2.80930E-04, -5.78626E-02,
                    5.86380E-01,  4.71202E-01 )
   ..
$LIBRARY-ENTRY Residential Fix Vol-Fan EIR     CURVE-FIT       Fan EIR-FPLR    
   TYPE = LINEAR   INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.0, 0.0)
   ..
$LIBRARY-ENTRY COIL-BF-FFLOW-SPEC              CURVE-FIT       Coil BF-FFLOW   
   TYPE = LINEAR   INPUT-TYPE = COEFFICIENTS
   OUTPUT-MIN = 0.8   COEFFICIENTS = (0.33,0.67)
   ..
$LIBRARY-ENTRY PTAC_EIR_fPLR                   CURVE-FIT       Pkgd Terminal AC SYSTEM 182
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.125, 0.875, 0, 0)
  ..  
$LIBRARY-ENTRY Two-Speed Fan EIR fPLR          CURVE-FIT       Fan EIR-FPLR
   TYPE = LINEAR   INPUT-TYPE = COEFFICIENTS
   OUTPUT-MIN = 0.4   COEFFICIENTS = (-0.764706,1.764706)
   ..
$LIBRARY-ENTRY ScrewH2OVSD-EIR-fCHWT&ECT       CURVE-FIT       Chiller EIR-fT
   TYPE             = BI-QUADRATIC-T
   INPUT-TYPE       = COEFFICIENTS
   COEFFICIENTS     = ( 0.121359, 0, 5.11244e-005, 0.0124407, 0.000137152, 
         -0.00033923 )
   ..
$LIBRARY-ENTRY ScrewH2OVSD-EIR-fPLR&dT         CURVE-FIT       Chiller EIR-fPLR&DT
   TYPE             = BI-QUADRATIC-RATIO&DT
   INPUT-TYPE       = COEFFICIENTS
   COEFFICIENTS     = ( 0.116358336, 0.358568939, 0.542210569, 
      -0.00148115, 5.12369E-05, -0.001037557 )
   ..
$LIBRARY-ENTRY ScrewH2OVSD-Cap-fCHW&ECT        CURVE-FIT       Chiller CAP-fT
   TYPE             = BI-QUADRATIC-T
   INPUT-TYPE       = COEFFICIENTS
   COEFFICIENTS     = ( 0.180282, 0, -0.000886407, 0.0172435, -0.00041915, 
         0.00109584 )
   ..

