$LIBRARY-ENTRY Mat_FlrJoistEnclosed            MATERIAL        UFlrCore
$ Description: Joist and cavity average properties
   TYPE = PROPERTIES
   THICKNESS = 0.625
   CONDUCTIVITY = 0.6188
   DENSITY = 3.2
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_FlrJoistOpen                MATERIAL        UFlrCore
$ Description: Joist and cavity average properties
   TYPE = PROPERTIES
   THICKNESS = 0.625
   CONDUCTIVITY = 11.2567
   DENSITY = 3.2
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_2X4MSplt                    MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.1458
   CONDUCTIVITY = 0.0666
   DENSITY = 32.0073
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_2X6MSplt                    MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.2292
   CONDUCTIVITY = 0.0666
   DENSITY = 31.9953
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_2X4_16                      MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.2917
   CONDUCTIVITY = 0.2537
   DENSITY = 7.9991
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_2X6_16                      MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.4583
   CONDUCTIVITY = 0.3917
   DENSITY = 8.0006
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_2X8_16                      MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.625
   CONDUCTIVITY = 0.5252
   DENSITY = 8
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_Stud_EW2X4                  MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.2917
   CONDUCTIVITY = 0.0354
   DENSITY = 10.2488
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY Mat_Stud_EW2X6                  MATERIAL        UFlrCore
$ Description: Stud and cavity average
   TYPE = PROPERTIES
   THICKNESS = 0.4583
   CONDUCTIVITY = 0.0354
   DENSITY = 10.2507
   SPECIFIC-HEAT = 0.33
   ..
$LIBRARY-ENTRY UFMat_Core                      MATERIAL        UFlrCore
$ Description: High resistance layer for core slabs
   TYPE = RESISTANCE
   RESISTANCE = 1000
   ..
$LIBRARY-ENTRY Mat_InsLay_EWall                MATERIAL        UFlrCore
$ Description: Exterior wall insulation layer
   TYPE = RESISTANCE
   RESISTANCE = { if(#PA("ComEWInsCalc") == "FromUo") then
 1/#PA("ComEWUo") - #PA("ComEWLayR") else #PA("ComEWInsR") endif}
   ..
$LIBRARY-ENTRY Mat_InsLay_AttFlr               MATERIAL        UFlrCore
$ Description: Attic floor insulation layer
   TYPE = RESISTANCE
   RESISTANCE = {#PA("AttFlrInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_Roof                 MATERIAL        UFlrCore
$ Description: Roof insulation layer
   TYPE = RESISTANCE
   RESISTANCE = { if(#PA("ComRoofInsCalc") == "FromUo") then
 1/#PA("ComRoofUo") - #PA("ComRoofLayR") else #PA("ComRoofInsR") endif}
   ..
$LIBRARY-ENTRY Mat_InsLay_AtticRoof            MATERIAL        UFlrCore
$ Description: Roof insulation layer
   TYPE = RESISTANCE
   RESISTANCE = {#PA("AtticRoofInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_FlrAbvCrawl          MATERIAL        UFlrCore
$ Description: Insulation in floor above crawl space
   TYPE = RESISTANCE
   RESISTANCE = {#PA("FlrAbvCrawlInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_DwlgEWall            MATERIAL        UFlrCore
$ Description: Exterior wall insulation layer
   TYPE = RESISTANCE
   RESISTANCE = { if(#PA("DwlgEWInsCalc") == "FromUo") then
 1/#PA("DwlgEWUo") - #PA("DwlgEWLayR") else #PA("DwlgEWInsR") endif}
   ..
$LIBRARY-ENTRY Mat_InsLay_DwlgRoof             MATERIAL        UFlrCore
$ Description: Roof insulation layer
   TYPE = RESISTANCE
   RESISTANCE = { if(#PA("DwlgRoofInsCalc") == "FromUo") then
 1/#PA("DwlgRoofUo") - #PA("DwlgRoofLayR") else #PA("DwlgRoofInsR") endif}
   ..
$LIBRARY-ENTRY Mat_InsLay_IWallFreezer         MATERIAL        UFlrCore
$ Description: Freezer wall to interior
   TYPE = RESISTANCE
   RESISTANCE = {#PA("IWallFreezerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_EWallFreezer         MATERIAL        UFlrCore
$ Description: Freezer wall to outdoors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("EWallFreezerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_RoofFreezer          MATERIAL        UFlrCore
$ Description: Freezer roof; may be interior or exterior
   TYPE = RESISTANCE
   RESISTANCE = {#PA("RoofFreezerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_FlrFreezer           MATERIAL        UFlrCore
$ Description: Freezer floor
   TYPE = RESISTANCE
   RESISTANCE = {#PA("FlrFreezerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_EWallCooler          MATERIAL        UFlrCore
$ Description: Cooler wall to interior
   TYPE = RESISTANCE
   RESISTANCE = {#PA("EWallCoolerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_IWallCooler          MATERIAL        UFlrCore
$ Description: Cooler wall to outdoors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("IWallCoolerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_RoofCooler           MATERIAL        UFlrCore
$ Description: Cooler roof int/ext
   TYPE = RESISTANCE
   RESISTANCE = {#PA("RoofCoolerInsR")}
   ..
$LIBRARY-ENTRY Mat_InsLay_FlrCooler            MATERIAL        UFlrCore
$ Description: Cooler floor
   TYPE = RESISTANCE
   RESISTANCE = {#PA("FlrCoolerInsR")}
   ..
$LIBRARY-ENTRY Mat_UFlrEdgeCC12                MATERIAL        UFlrCore
$ Description: Perimiter strip resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = 1000
   ..
$LIBRARY-ENTRY Mat_UFlrEdgeCC06Carpet          MATERIAL        UFlrCore
$ Description: Perimiter strip resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = 1000
   ..
$LIBRARY-ENTRY Mat_UFlrEdgeCC04Carpet          MATERIAL        UFlrCore
$ Description: Perimiter strip resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = 1000
   ..
$LIBRARY-ENTRY Mat_UFlrEdgeCC04Tile            MATERIAL        UFlrCore
$ Description: Perimiter strip resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = 1000
   ..
$LIBRARY-ENTRY Mat_UFlrEdgeCC06Tile            MATERIAL        UFlrCore
$ Description: Perimiter strip resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = 1000
   ..
$LIBRARY-ENTRY Mat_UFictDirt01                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt01")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt02                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt02")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt03                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt03")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt04                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt04")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt05                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt05")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt06                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt06")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt07                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt07")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt08                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt08")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt09                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt09")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt10                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt10")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt11                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt11")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt12                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt12")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt13                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt13")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt14                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt14")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt15                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt15")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt16                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt16")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt17                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt17")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt18                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt18")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt19                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt19")}
   ..
$LIBRARY-ENTRY Mat_UFictDirt20                 MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_Dirt20")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile01             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile01")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile02             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile02")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile03             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile03")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile04             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile04")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile05             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile05")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile06             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile06")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile07             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile07")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile08             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile08")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile09             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile09")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile10             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile10")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile11             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile11")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile12             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile12")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile13             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile13")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile14             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile14")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile15             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile15")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile16             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile16")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile17             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile17")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile18             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile18")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile19             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile19")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Tile20             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Tile20")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet01           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet01")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet02           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet02")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet03           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet03")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet04           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet04")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet05           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet05")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet06           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet06")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet07           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet07")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet08           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet08")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet09           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet09")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet10           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet10")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet11           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet11")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet12           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet12")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet13           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet13")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet14           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet14")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet15           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet15")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet16           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet16")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet17           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet17")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet18           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet18")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet19           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet19")}
   ..
$LIBRARY-ENTRY Mat_UFictCC04Carpet20           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC04Carpet20")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile01             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile01")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile02             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile02")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile03             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile03")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile04             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile04")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile05             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile05")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile06             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile06")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile07             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile07")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile08             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile08")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile09             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile09")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile10             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile10")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile11             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile11")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile12             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile12")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile13             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile13")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile14             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile14")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile15             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile15")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile16             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile16")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile17             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile17")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile18             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile18")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile19             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile19")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Tile20             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Tile20")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet01           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet01")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet02           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet02")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet03           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet03")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet04           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet04")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet05           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet05")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet06           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet06")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet07           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet07")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet08           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet08")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet09           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet09")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet10           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet10")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet11           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet11")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet12           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet12")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet13           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet13")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet14           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet14")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet15           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet15")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet16           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet16")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet17           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet17")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet18           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet18")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet19           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet19")}
   ..
$LIBRARY-ENTRY Mat_UFictCC06Carpet20           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC06Carpet20")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile01             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile01")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile02             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile02")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile03             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile03")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile04             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile04")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile05             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile05")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile06             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile06")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile07             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile07")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile08             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile08")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile09             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile09")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile10             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile10")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile11             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile11")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile12             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile12")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile13             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile13")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile14             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile14")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile15             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile15")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile16             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile16")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile17             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile17")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile18             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile18")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile19             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile19")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Tile20             MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Tile20")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet01           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet01")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet02           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet02")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet03           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet03")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet04           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet04")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet05           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet05")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet06           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet06")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet07           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet07")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet08           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet08")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet09           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet09")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet10           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet10")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet11           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet11")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet12           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet12")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet13           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet13")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet14           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet14")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet15           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet15")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet16           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet16")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet17           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet17")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet18           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet18")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet19           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet19")}
   ..
$LIBRARY-ENTRY Mat_UFictCC12Carpet20           MATERIAL        UFlrCore
$ Description: Fictitious resistance layer for slab floors
   TYPE = RESISTANCE
   RESISTANCE = {#PA("UFR_CC12Carpet20")}
   ..
$LIBRARY-ENTRY Lay_ClgBelowPlnmCom             LAYERS          Ceiling
$ Description: Ceiling below plnm, nonres; 1/2 inch Clg tile + 2 air films/ht fl
   MATERIAL = (
      "AcousTile (HF-E5)")
   ..
$LIBRARY-ENTRY Cons_ClgBelowPlnmCom            CONSTRUCTION    Ceiling
$ Description: Ceiling below plnm, nonres; 1/2 inch Clg tile + 2 air films/ht fl
   TYPE = LAYERS
   LAYERS = Lay_ClgBelowPlnmCom
   ..
$LIBRARY-ENTRY Cons_ClgBelowPlnmRes            CONSTRUCTION    Ceiling
$ Description: Ceiling below plnm, residential; 1/2 in gypbd + joists w/ air fil
   TYPE = U-VALUE
   U-VALUE = 0.552
   ..
$LIBRARY-ENTRY Lay_ClgConc                     LAYERS          Clg
$ Description: Ceiling w/o plenum, concrete
   MATERIAL = (
      "Conc HW 140lb 6in (HF-C13)")
   ..
$LIBRARY-ENTRY Cons_ClgConc                    CONSTRUCTION    Clg
$ Description: Ceiling w/o plenum, concrete
   TYPE = LAYERS
   LAYERS = Lay_ClgConc
   ..
$LIBRARY-ENTRY Lay_ClgLite                     LAYERS          Clg
$ Description: Ceiling w/o plenum, light; Has cavity
   MATERIAL = (
      "Carpet & Rubber Pad (CP02)","Plywd 1in (PW06)",
      "Mat_FlrJoistEnclosed","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_ClgLite                    CONSTRUCTION    Clg
$ Description: Ceiling w/o plenum, light; Has cavity
   TYPE = LAYERS
   LAYERS = Lay_ClgLite
   ..
$LIBRARY-ENTRY Cons_WoodDoor                   CONSTRUCTION    Door
$ Description: 2.25inch solid core flush, no storm
   TYPE = U-VALUE
   U-VALUE = 0.69
   ..
$LIBRARY-ENTRY Cons_GarageDoor                 CONSTRUCTION    DoorGar
$ Description: Garage door
   TYPE = U-VALUE
   U-VALUE = 2.1
   ..
$LIBRARY-ENTRY Cons_OpenDoorway                CONSTRUCTION    DoorIntOpen
$ Description: Open interior doorway; Air wall
   TYPE = U-VALUE
   U-VALUE = 2.7
   ..
$LIBRARY-ENTRY Cons_DoorUninsMtl               CONSTRUCTION    DoorUninsMtl
$ Description: Uninsulated metal door
   TYPE = U-VALUE
   U-VALUE = 0.82
   ..
$LIBRARY-ENTRY Cons_DoorU0p56                  CONSTRUCTION    Door
$ Description: 2.25inch solid core flush, no storm
   TYPE = U-VALUE
   U-VALUE = 0.56
   ..
$LIBRARY-ENTRY Cons_DoorU0p53                  CONSTRUCTION    Door
$ Description: 2.25inch solid core flush, no storm
   TYPE = U-VALUE
   U-VALUE = 0.53
   ..
$LIBRARY-ENTRY Cons_DoorU0p23                  CONSTRUCTION    Door
$ Description: 2.25inch solid core flush, no storm
   TYPE = U-VALUE
   U-VALUE = 0.23
   ..
$LIBRARY-ENTRY Lay_AtticFlr                    LAYERS          Ceiling
$ Description: Lay_AtticFlr
   MATERIAL = (
      "Mat_InsLay_AttFlr","GypBd 5/8in (GP02)")
   ..
$LIBRARY-ENTRY Cons_AtticFlr                   CONSTRUCTION    Ceiling
$ Description: Lay_AtticFlr
   TYPE = LAYERS
   LAYERS = Lay_AtticFlr
   ..
$LIBRARY-ENTRY Lay_EWallSpandrel               LAYERS          EWall
$ Description: Lay_EWallSpandrel
   MATERIAL = (
      "1/4in Spandrel Glass","Bldg Paper Felt (BP01)",
      "Mat_InsLay_EWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_EWallSpandrel              CONSTRUCTION    EWall
$ Description: Lay_EWallSpandrel
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 6
   LAYERS = Lay_EWallSpandrel
   ..
$LIBRARY-ENTRY Lay_EWallConc                   LAYERS          EWall
$ Description: Lay_EWallConc
   MATERIAL = (
      "CMU MW 8in Hollow (CB31)","Mat_InsLay_EWall",
      "GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_EWallConc                  CONSTRUCTION    EWall
$ Description: Lay_EWallConc
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 2
   LAYERS = Lay_EWallConc
   ..
$LIBRARY-ENTRY Lay_EWallBrickConc              LAYERS          EWall
$ Description: Lay_EWallBrickConc
   MATERIAL = (
      "Face Brick 4in (BK05)","Mat_InsLay_EWall",
      "CMU MW 8in Hollow (CB31)")
   ..
$LIBRARY-ENTRY Cons_EWallBrickConc             CONSTRUCTION    EWall
$ Description: Lay_EWallBrickConc
   TYPE = LAYERS
   ABSORPTANCE = 0.88
   ROUGHNESS = 2
   LAYERS = Lay_EWallBrickConc
   ..
$LIBRARY-ENTRY Lay_EWallWoodFrm                LAYERS          EWall
$ Description: Lay_EWallWoodFrm
   MATERIAL = (
      "Plywd 5/8in (PW04)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_EWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_EWallWoodFrm               CONSTRUCTION    EWall
$ Description: Lay_EWallWoodFrm
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 4
   LAYERS = Lay_EWallWoodFrm
   ..
$LIBRARY-ENTRY Lay_EWallSteelSdg               LAYERS          EWall
$ Description: Lay_EWallSteelSdg
   MATERIAL = (
      "Steel Siding (AS01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_EWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_EWallSteelSdg              CONSTRUCTION    EWall
$ Description: Lay_EWallSteelSdg
   TYPE = LAYERS
   ABSORPTANCE = 0.8
   ROUGHNESS = 4
   LAYERS = Lay_EWallSteelSdg
   ..
$LIBRARY-ENTRY Lay_EWallStucco                 LAYERS          EWall
$ Description: Lay_EWallStucco
   MATERIAL = (
      "Stucco 1in (SC01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_EWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_EWallStucco                CONSTRUCTION    EWall
$ Description: Lay_EWallStucco
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_EWallStucco
   ..
$LIBRARY-ENTRY Lay_EWallStuccoNoIns            LAYERS          EWall
$ Description: Garage exterior wall
   MATERIAL = (
      "Stucco 1in (SC01)","Bldg Paper Felt (BP01)",
      "GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_EWallStuccoNoIns           CONSTRUCTION    EWall
$ Description: Garage exterior wall
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_EWallStuccoNoIns
   ..
$LIBRARY-ENTRY Cons_EWallGH                    CONSTRUCTION    EWall
$ Description: Massless wall for greenhouse
   TYPE = U-VALUE
   ROUGHNESS = 6
   U-VALUE = 1.1
   ..
$LIBRARY-ENTRY Lay_DwlgEWallSpandrel           LAYERS          EWall
$ Description: Lay_DwlgEWallSpandrel
   MATERIAL = (
      "1/4in Spandrel Glass","Bldg Paper Felt (BP01)",
      "Mat_InsLay_DwlgEWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_DwlgEWallSpandrel          CONSTRUCTION    EWall
$ Description: Lay_DwlgEWallSpandrel
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 6
   LAYERS = Lay_DwlgEWallSpandrel
   ..
$LIBRARY-ENTRY Lay_DwlgEWallStucco             LAYERS          EWall
$ Description: Lay_DwlgEWallStucco
   MATERIAL = (
      "Stucco 1in (SC01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_DwlgEWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_DwlgEWallStucco            CONSTRUCTION    EWall
$ Description: Lay_DwlgEWallStucco
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_DwlgEWallStucco
   ..
$LIBRARY-ENTRY Lay_IFlrCC04Carpet              LAYERS          IFlr
$ Description: Lay_IFlrCC04Carpet
   MATERIAL = (
      "Conc HW 140lb 4in (HF-C5)","Carpet & No Pad")
   ..
$LIBRARY-ENTRY Cons_IFlrCC04Carpet             CONSTRUCTION    IFlr
$ Description: Lay_IFlrCC04Carpet
   TYPE = LAYERS
   LAYERS = Lay_IFlrCC04Carpet
   ..
$LIBRARY-ENTRY Lay_IFlrCC06Carpet              LAYERS          IFlr
$ Description: Lay_IFlrCC06Carpet
   MATERIAL = (
      "Conc HW 140lb 6in (HF-C13)","Carpet & No Pad")
   ..
$LIBRARY-ENTRY Cons_IFlrCC06Carpet             CONSTRUCTION    IFlr
$ Description: Lay_IFlrCC06Carpet
   TYPE = LAYERS
   LAYERS = Lay_IFlrCC06Carpet
   ..
$LIBRARY-ENTRY Lay_IFlrCC12Carpet              LAYERS          IFlr
$ Description: Lay_IFlrCC12Carpet
   MATERIAL = (
      "Conc HW 140lb 12in (HF-C11)","Carpet & No Pad")
   ..
$LIBRARY-ENTRY Cons_IFlrCC12Carpet             CONSTRUCTION    IFlr
$ Description: Lay_IFlrCC12Carpet
   TYPE = LAYERS
   LAYERS = Lay_IFlrCC12Carpet
   ..
$LIBRARY-ENTRY Lay_IFlrCC04Tile                LAYERS          IFlr
$ Description: Lay_IFlrCC04Tile
   MATERIAL = (
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_IFlrCC04Tile               CONSTRUCTION    IFlr
$ Description: Lay_IFlrCC04Tile
   TYPE = LAYERS
   LAYERS = Lay_IFlrCC04Tile
   ..
$LIBRARY-ENTRY Lay_IFlrCC06Tile                LAYERS          IFlr
$ Description: Lay_IFlrCC06Tile
   MATERIAL = (
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_IFlrCC06Tile               CONSTRUCTION    IFlr
$ Description: Lay_IFlrCC06Tile
   TYPE = LAYERS
   LAYERS = Lay_IFlrCC06Tile
   ..
$LIBRARY-ENTRY Lay_IFlrCC12Tile                LAYERS          IFlr
$ Description: Lay_IFlrCC12Tile
   MATERIAL = (
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_IFlrCC12Tile               CONSTRUCTION    IFlr
$ Description: Lay_IFlrCC12Tile
   TYPE = LAYERS
   LAYERS = Lay_IFlrCC12Tile
   ..
$LIBRARY-ENTRY Lay_IFlrConcCarpet              LAYERS          IFlr
$ Description: Lay_IFlrConcCarpet
   MATERIAL = (
      "Conc HW 140lb 4in (HF-C5)","Carpet & No Pad")
   ..
$LIBRARY-ENTRY Cons_IFlrConcCarpet             CONSTRUCTION    IFlr
$ Description: Lay_IFlrConcCarpet
   TYPE = LAYERS
   LAYERS = Lay_IFlrConcCarpet
   ..
$LIBRARY-ENTRY Lay_IFlrConcBare                LAYERS          IFlr
$ Description: Lay_IFlrConcBare
   MATERIAL = (
      "Conc HW 140lb 6in (HF-C13)")
   ..
$LIBRARY-ENTRY Cons_IFlrConcBare               CONSTRUCTION    IFlr
$ Description: Lay_IFlrConcBare
   TYPE = LAYERS
   LAYERS = Lay_IFlrConcBare
   ..
$LIBRARY-ENTRY Lay_IFlrWoodGyp                 LAYERS          IFlr
$ Description: Has cavity
   MATERIAL = (
      "GypBd 1/2in (GP01)","Mat_FlrJoistEnclosed",
      "Plywd 1in (PW06)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_IFlrWoodGyp                CONSTRUCTION    IFlr
$ Description: Has cavity
   TYPE = LAYERS
   LAYERS = Lay_IFlrWoodGyp
   ..
$LIBRARY-ENTRY Lay_IFlrWoodOpen                LAYERS          IFlr
$ Description: No cavity
   MATERIAL = (
      "Mat_FlrJoistOpen","Plywd 1in (PW06)",
      "Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_IFlrWoodOpen               CONSTRUCTION    IFlr
$ Description: No cavity
   TYPE = LAYERS
   LAYERS = Lay_IFlrWoodOpen
   ..
$LIBRARY-ENTRY Lay_IWallLite                   LAYERS          IWall
$ Description: Lay_IWallLite
   MATERIAL = (
      "GypBd 1/2in (GP01)","Mat_2X4_16",
      "GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_IWallLite                  CONSTRUCTION    IWall
$ Description: Lay_IWallLite
   TYPE = LAYERS
   LAYERS = Lay_IWallLite
   ..
$LIBRARY-ENTRY Lay_IWallCMU6                   LAYERS          IWall
$ Description: Lay_IWallCMU6
   MATERIAL = (
      "CMU MW 6in Hollow (CB26)")
   ..
$LIBRARY-ENTRY Cons_IWallCMU6                  CONSTRUCTION    IWall
$ Description: Lay_IWallCMU6
   TYPE = LAYERS
   LAYERS = Lay_IWallCMU6
   ..
$LIBRARY-ENTRY Lay_IWallToAttic                LAYERS          IWall
$ Description: Insulated interior wall to uncond attic; same insulation layer as
   MATERIAL = (
      "Plywd 5/8in (PW04)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_EWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_IWallToAttic               CONSTRUCTION    IWall
$ Description: Insulated interior wall to uncond attic; same insulation layer as
   TYPE = LAYERS
   LAYERS = Lay_IWallToAttic
   ..
$LIBRARY-ENTRY Lay_IWallToGar                  LAYERS          IWall
$ Description: Insulated interior wall to uncond garage; same insulation layer a
   MATERIAL = (
      "Plywd 5/8in (PW04)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_EWall","GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_IWallToGar                 CONSTRUCTION    IWall
$ Description: Insulated interior wall to uncond garage; same insulation layer a
   TYPE = LAYERS
   LAYERS = Lay_IWallToGar
   ..
$LIBRARY-ENTRY Cons_AirWall                    CONSTRUCTION    Air Wall
$ Description: $
   TYPE = U-VALUE
   U-VALUE = 2.7
   ..
$LIBRARY-ENTRY Lay_RoofSteel                   LAYERS          Roof
$ Description: Lay_RoofSteel
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_Roof","Steel Siding (AS01)")
   ..
$LIBRARY-ENTRY Cons_RoofSteel                  CONSTRUCTION    Roof
$ Description: Lay_RoofSteel
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_RoofSteel
   ..
$LIBRARY-ENTRY Lay_RoofPlywdIns                LAYERS          Roof
$ Description: Lay_RoofPlywdIns
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_Roof","Plywd 5/8in (PW04)",
      "GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_RoofPlywdIns               CONSTRUCTION    Roof
$ Description: Lay_RoofPlywdIns
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_RoofPlywdIns
   ..
$LIBRARY-ENTRY Lay_RoofConc                    LAYERS          Roof
$ Description: Lay_RoofConc
   MATERIAL = (
      "Bldg Paper Felt (BP01)","Mat_InsLay_Roof",
      "Conc HW 140lb 4in (CC03)")
   ..
$LIBRARY-ENTRY Cons_RoofConc                   CONSTRUCTION    Roof
$ Description: Lay_RoofConc
   TYPE = LAYERS
   LAYERS = Lay_RoofConc
   ..
$LIBRARY-ENTRY Lay_DwlgRoofSteel               LAYERS          Roof
$ Description: Lay_DwlgRoofSteel
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_DwlgRoof","Steel Siding (AS01)")
   ..
$LIBRARY-ENTRY Cons_DwlgRoofSteel              CONSTRUCTION    Roof
$ Description: Lay_DwlgRoofSteel
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_DwlgRoofSteel
   ..
$LIBRARY-ENTRY Lay_DwlgRoofPlwdIns             LAYERS          Roof
$ Description: Lay_DwlgRoofPlwdIns
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_DwlgRoof","Plywd 5/8in (PW04)",
      "GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_DwlgRoofPlwdIns            CONSTRUCTION    Roof
$ Description: Lay_DwlgRoofPlwdIns
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_DwlgRoofPlwdIns
   ..
$LIBRARY-ENTRY Lay_DwlgRoofConc                LAYERS          Roof
$ Description: Lay_DwlgRoofConc
   MATERIAL = (
      "Bldg Paper Felt (BP01)","Mat_InsLay_DwlgRoof",
      "Conc HW 140lb 4in (CC03)")
   ..
$LIBRARY-ENTRY Cons_DwlgRoofConc               CONSTRUCTION    Roof
$ Description: Lay_DwlgRoofConc
   TYPE = LAYERS
   LAYERS = Lay_DwlgRoofConc
   ..
$LIBRARY-ENTRY Lay_RoofCathIns                 LAYERS          Roof
$ Description: Lay_RoofCathIns
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Plywd 5/8in (PW04)","Mat_InsLay_Roof",
      "GypBd 1/2in (GP01)")
   ..
$LIBRARY-ENTRY Cons_RoofCathIns                CONSTRUCTION    Roof
$ Description: Lay_RoofCathIns
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_RoofCathIns
   ..
$LIBRARY-ENTRY Lay_RoofPlywdNoIns              LAYERS          Roof
$ Description: For garage
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Plywd 3/4in (PW05)")
   ..
$LIBRARY-ENTRY Cons_RoofPlywdNoIns             CONSTRUCTION    Roof
$ Description: For garage
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_RoofPlywdNoIns
   ..
$LIBRARY-ENTRY Lay_RoofAtticNoIns              LAYERS          Roof
$ Description: Lay_RoofAtticNoIns
   INSIDE-FILM-RES = {1/(1/#PA("RoofInsideRConv")+#PA("RoofInsideEmiss"))}
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Plywd 3/4in (PW05)")
   ..
$LIBRARY-ENTRY Cons_RoofAtticNoIns             CONSTRUCTION    Roof
$ Description: Lay_RoofAtticNoIns
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_RoofAtticNoIns
   ..
$LIBRARY-ENTRY Lay_RoofAtticIns                LAYERS          Roof
$ Description: Lay_RoofAtticIns
   INSIDE-FILM-RES = {1/(1/#PA("RoofInsideRConv")+#PA("RoofInsideEmiss"))}
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Bldg Paper Felt (BP01)",
      "Mat_InsLay_AtticRoof","Plywd 3/4in (PW05)")
   ..
$LIBRARY-ENTRY Cons_RoofAtticIns               CONSTRUCTION    Roof
$ Description: Lay_RoofAtticIns
   TYPE = LAYERS
   ABSORPTANCE = 0.6
   ROUGHNESS = 1
   LAYERS = Lay_RoofAtticIns
   ..
$LIBRARY-ENTRY Lay_RoofTileIns                 LAYERS          Roof
$ Description: Lay_RoofTileIns
   INSIDE-FILM-RES = {1/(1/#PA("RoofInsideRConv")+#PA("RoofInsideEmiss"))}
   MATERIAL = (
      "ClayTile Paver 3/8in (CT11)","Blt-Up Roof 3/8in (BR01)",
      "Bldg Paper Felt (BP01)","Plywd 3/4in (PW05)",
      "Mat_InsLay_AtticRoof")
   ..
$LIBRARY-ENTRY Cons_RoofTileIns                CONSTRUCTION    Roof
$ Description: Lay_RoofTileIns
   TYPE = LAYERS
   ABSORPTANCE = 0.58
   ROUGHNESS = 3
   LAYERS = Lay_RoofTileIns
   ..
$LIBRARY-ENTRY Lay_RoofTileNoIns               LAYERS          Roof
$ Description: Lay_RoofTileNoIns
   INSIDE-FILM-RES = {1/(1/#PA("RoofInsideRConv")+#PA("RoofInsideEmiss"))}
   MATERIAL = (
      "ClayTile Paver 3/8in (CT11)","Blt-Up Roof 3/8in (BR01)",
      "Bldg Paper Felt (BP01)","Plywd 3/4in (PW05)")
   ..
$LIBRARY-ENTRY Cons_RoofTileNoIns              CONSTRUCTION    Roof
$ Description: Lay_RoofTileNoIns
   TYPE = LAYERS
   ABSORPTANCE = 0.58
   ROUGHNESS = 3
   LAYERS = Lay_RoofTileNoIns
   ..
$LIBRARY-ENTRY Lay_RoofShngIns                 LAYERS          Roof
$ Description: Lay_RoofShngIns
   INSIDE-FILM-RES = {1/(1/#PA("RoofInsideRConv")+#PA("RoofInsideEmiss"))}
   MATERIAL = (
      "Wood Shingle (WS02)","Blt-Up Roof 3/8in (BR01)",
      "Bldg Paper Felt (BP01)","Plywd 3/4in (PW05)",
      "Mat_InsLay_AtticRoof")
   ..
$LIBRARY-ENTRY Cons_RoofShngIns                CONSTRUCTION    Roof
$ Description: Lay_RoofShngIns
   TYPE = LAYERS
   ABSORPTANCE = 0.88
   ROUGHNESS = 2
   LAYERS = Lay_RoofShngIns
   ..
$LIBRARY-ENTRY Lay_RoofShngNoIns               LAYERS          Roof
$ Description: Lay_RoofShngNoIns
   INSIDE-FILM-RES = {1/(1/#PA("RoofInsideRConv")+#PA("RoofInsideEmiss"))}
   MATERIAL = (
      "Wood Shingle (WS02)","Blt-Up Roof 3/8in (BR01)",
      "Bldg Paper Felt (BP01)","Plywd 3/4in (PW05)")
   ..
$LIBRARY-ENTRY Cons_RoofShngNoIns              CONSTRUCTION    Roof
$ Description: Lay_RoofShngNoIns
   TYPE = LAYERS
   ABSORPTANCE = 0.88
   ROUGHNESS = 2
   LAYERS = Lay_RoofShngNoIns
   ..
$LIBRARY-ENTRY Lay_Crawl_Flr                   LAYERS          CrawlFlr
$ Description: Lay_Crawl_Flr
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_Crawl_Flr                  CONSTRUCTION    CrawlFlr
$ Description: Lay_Crawl_Flr
   TYPE = LAYERS
   LAYERS = Lay_Crawl_Flr
   ..
$LIBRARY-ENTRY Lay_Crawl_Wall                  LAYERS          CrawlWall
$ Description: Lay_Crawl_Wall
   MATERIAL = (
      "Plywd 1in (PW06)")
   ..
$LIBRARY-ENTRY Cons_Crawl_Wall                 CONSTRUCTION    CrawlWall
$ Description: Lay_Crawl_Wall
   TYPE = LAYERS
   LAYERS = Lay_Crawl_Wall
   ..
$LIBRARY-ENTRY Lay_Crawl_Abv                   LAYERS          CrawlAbv
$ Description: Lay_Crawl_Abv
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_InsLay_FlrAbvCrawl","Plywd 1in (PW06)",
      "Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_Crawl_Abv                  CONSTRUCTION    CrawlAbv
$ Description: Lay_Crawl_Abv
   TYPE = LAYERS
   LAYERS = Lay_Crawl_Abv
   ..
$LIBRARY-ENTRY Lay_UFlrCoreCC12                LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "UFMat_Core","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)")
   ..
$LIBRARY-ENTRY Cons_UFlrCoreCC12               CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrCoreCC12
   ..
$LIBRARY-ENTRY Lay_UFlrCoreCC06Carpet          LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "UFMat_Core","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & No Pad")
   ..
$LIBRARY-ENTRY Cons_UFlrCoreCC06Carpet         CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrCoreCC06Carpet
   ..
$LIBRARY-ENTRY Lay_UFlrCoreCC04Carpet          LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "UFMat_Core","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFlrCoreCC04Carpet         CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrCoreCC04Carpet
   ..
$LIBRARY-ENTRY Lay_UFlrCoreCC04Tile            LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "UFMat_Core","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFlrCoreCC04Tile           CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrCoreCC04Tile
   ..
$LIBRARY-ENTRY Lay_UFlrCoreCC06Tile            LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "UFMat_Core","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFlrCoreCC06Tile           CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrCoreCC06Tile
   ..
$LIBRARY-ENTRY Lay_UFlrEdgeCC12                LAYERS          UFlrEdge
$ Description: Perimeter slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFlrEdgeCC12","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)")
   ..
$LIBRARY-ENTRY Cons_UFlrEdgeCC12               CONSTRUCTION    UFlrEdge
$ Description: Perimeter slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrEdgeCC12
   ..
$LIBRARY-ENTRY Lay_UFlrEdgeCC06Carpet          LAYERS          UFlrEdge
$ Description: Perimeter slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFlrEdgeCC06Carpet","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFlrEdgeCC06Carpet         CONSTRUCTION    UFlrEdge
$ Description: Perimeter slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrEdgeCC06Carpet
   ..
$LIBRARY-ENTRY Lay_UFlrEdgeCC04Carpet          LAYERS          UFlrEdge
$ Description: Perimeter slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFlrEdgeCC04Carpet","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFlrEdgeCC04Carpet         CONSTRUCTION    UFlrEdge
$ Description: Perimeter slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrEdgeCC04Carpet
   ..
$LIBRARY-ENTRY Lay_UFlrEdgeCC04Tile            LAYERS          UFlrEdge
$ Description: Perimeter slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFlrEdgeCC04Tile","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFlrEdgeCC04Tile           CONSTRUCTION    UFlrEdge
$ Description: Perimeter slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrEdgeCC04Tile
   ..
$LIBRARY-ENTRY Lay_UFlrEdgeCC06Tile            LAYERS          UFlrEdge
$ Description: Perimeter slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFlrEdgeCC06Tile","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFlrEdgeCC06Tile           CONSTRUCTION    UFlrEdge
$ Description: Perimeter slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFlrEdgeCC06Tile
   ..
$LIBRARY-ENTRY Cons_SlabEdge                   CONSTRUCTION    UFlrEdge
$ Description: Perimeter slab on ground
   TYPE = U-VALUE
   ROUGHNESS = 6
   U-VALUE = 0.8334
   ..
$LIBRARY-ENTRY Lay_IWallFreezer                LAYERS          IWall
$ Description: Freezer IWall
   INSIDE-FILM-RES = 0.68
   MATERIAL = (
      "Steel Siding (HF-A3)","Plywd 5/8in (PW04)",
      "Mat_InsLay_IWallFreezer","Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_IWallFreezer               CONSTRUCTION    IWall
$ Description: Freezer IWall
   TYPE = LAYERS
   LAYERS = Lay_IWallFreezer
   ..
$LIBRARY-ENTRY Lay_EWallFreezer                LAYERS          EWall
$ Description: Freezer EWall
   INSIDE-FILM-RES = 0.68
   MATERIAL = (
      "Conc HW 140lb 6in (CC04)","Mat_InsLay_EWallFreezer",
      "Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_EWallFreezer               CONSTRUCTION    EWall
$ Description: Freezer EWall
   TYPE = LAYERS
   LAYERS = Lay_EWallFreezer
   ..
$LIBRARY-ENTRY Lay_RoofFreezer                 LAYERS          Roof
$ Description: Freezer roof
   INSIDE-FILM-RES = 0.62
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Plywd 5/8in (PW04)",
      "Mat_InsLay_RoofFreezer","Polyurethane 1 1/2in",
      "Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_RoofFreezer                CONSTRUCTION    Roof
$ Description: Freezer roof
   TYPE = LAYERS
   LAYERS = Lay_RoofFreezer
   ..
$LIBRARY-ENTRY Lay_FlrFreezer                  LAYERS          Floor
$ Description: Freezer floor
   INSIDE-FILM-RES = 0.92
   MATERIAL = (
      "Soil 12in","Conc HW 140lb 6in (HF-C13)",
      "Mat_InsLay_FlrFreezer","Polyurethane 1/2in (IN41)",
      "Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_FlrFreezer                 CONSTRUCTION    Floor
$ Description: Freezer floor
   TYPE = LAYERS
   LAYERS = Lay_FlrFreezer
   ..
$LIBRARY-ENTRY Lay_RoofCooler                  LAYERS          Roof
$ Description: Cooler roof
   INSIDE-FILM-RES = 0.62
   MATERIAL = (
      "Blt-Up Roof 3/8in (BR01)","Plywd 5/8in (PW04)",
      "Mat_InsLay_RoofCooler","Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_RoofCooler                 CONSTRUCTION    Roof
$ Description: Cooler roof
   TYPE = LAYERS
   LAYERS = Lay_RoofCooler
   ..
$LIBRARY-ENTRY Lay_IWallCooler                 LAYERS          IWall
$ Description: Cooler IWall
   INSIDE-FILM-RES = 0.68
   MATERIAL = (
      "Steel Siding (HF-A3)","Plywd 5/8in (PW04)",
      "Mat_InsLay_IWallCooler","Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_IWallCooler                CONSTRUCTION    IWall
$ Description: Cooler IWall
   TYPE = LAYERS
   LAYERS = Lay_IWallCooler
   ..
$LIBRARY-ENTRY Lay_EWallCooler                 LAYERS          EWall
$ Description: Cooler EWall
   MATERIAL = (
      "Conc HW 140lb 6in (CC04)","Mat_InsLay_EWallCooler",
      "Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_EWallCooler                CONSTRUCTION    EWall
$ Description: Cooler EWall
   TYPE = LAYERS
   LAYERS = Lay_EWallCooler
   ..
$LIBRARY-ENTRY Lay_FlrCooler                   LAYERS          Floor
$ Description: Cooler floor
   INSIDE-FILM-RES = 0.92
   MATERIAL = (
      "Soil 12in","Conc HW 140lb 6in (HF-C13)",
      "Mat_InsLay_FlrCooler","Steel Siding (HF-A3)")
   ..
$LIBRARY-ENTRY Cons_FlrCooler                  CONSTRUCTION    Floor
$ Description: Cooler floor
   TYPE = LAYERS
   LAYERS = Lay_FlrCooler
   ..
$LIBRARY-ENTRY Lay_UFictDirt01                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt01","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt01                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt01
   ..
$LIBRARY-ENTRY Lay_UFictDirt02                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt02","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt02                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt02
   ..
$LIBRARY-ENTRY Lay_UFictDirt03                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt03","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt03                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt03
   ..
$LIBRARY-ENTRY Lay_UFictDirt04                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt04","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt04                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt04
   ..
$LIBRARY-ENTRY Lay_UFictDirt05                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt05","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt05                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt05
   ..
$LIBRARY-ENTRY Lay_UFictDirt06                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt06","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt06                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt06
   ..
$LIBRARY-ENTRY Lay_UFictDirt07                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt07","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt07                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt07
   ..
$LIBRARY-ENTRY Lay_UFictDirt08                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt08","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt08                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt08
   ..
$LIBRARY-ENTRY Lay_UFictDirt09                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt09","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt09                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt09
   ..
$LIBRARY-ENTRY Lay_UFictDirt10                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt10","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt10                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt10
   ..
$LIBRARY-ENTRY Lay_UFictDirt11                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt11","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt11                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt11
   ..
$LIBRARY-ENTRY Lay_UFictDirt12                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt12","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt12                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt12
   ..
$LIBRARY-ENTRY Lay_UFictDirt13                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt13","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt13                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt13
   ..
$LIBRARY-ENTRY Lay_UFictDirt14                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt14","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt14                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt14
   ..
$LIBRARY-ENTRY Lay_UFictDirt15                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt15","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt15                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt15
   ..
$LIBRARY-ENTRY Lay_UFictDirt16                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt16","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt16                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt16
   ..
$LIBRARY-ENTRY Lay_UFictDirt17                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt17","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt17                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt17
   ..
$LIBRARY-ENTRY Lay_UFictDirt18                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt18","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt18                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt18
   ..
$LIBRARY-ENTRY Lay_UFictDirt19                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt19","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt19                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt19
   ..
$LIBRARY-ENTRY Lay_UFictDirt20                 LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictDirt20","Light Soil, Damp 12in")
   ..
$LIBRARY-ENTRY Cons_UFictDirt20                CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictDirt20
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile01             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile01","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile01            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile01
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile02             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile02","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile02            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile02
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile03             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile03","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile03            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile03
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile04             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile04","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile04            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile04
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile05             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile05","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile05            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile05
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile06             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile06","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile06            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile06
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile07             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile07","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile07            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile07
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile08             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile08","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile08            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile08
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile09             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile09","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile09            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile09
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile10             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile10","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile10            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile10
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile11             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile11","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile11            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile11
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile12             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile12","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile12            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile12
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile13             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile13","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile13            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile13
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile14             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile14","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile14            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile14
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile15             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile15","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile15            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile15
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile16             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile16","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile16            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile16
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile17             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile17","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile17            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile17
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile18             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile18","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile18            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile18
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile19             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile19","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile19            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile19
   ..
$LIBRARY-ENTRY Lay_UFictCC04Tile20             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Tile20","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Tile20            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Tile20
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet01           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet01","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet01          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet01
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet02           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet02","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet02          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet02
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet03           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet03","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet03          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet03
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet04           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet04","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet04          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet04
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet05           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet05","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet05          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet05
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet06           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet06","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet06          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet06
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet07           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet07","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet07          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet07
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet08           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet08","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet08          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet08
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet09           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet09","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet09          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet09
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet10           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet10","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet10          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet10
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet11           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet11","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet11          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet11
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet12           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet12","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet12          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet12
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet13           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet13","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet13          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet13
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet14           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet14","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet14          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet14
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet15           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet15","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet15          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet15
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet16           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet16","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet16          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet16
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet17           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet17","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet17          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet17
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet18           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet18","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet18          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet18
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet19           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet19","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet19          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet19
   ..
$LIBRARY-ENTRY Lay_UFictCC04Carpet20           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC04Carpet20","Light Soil, Damp 12in",
      "Conc HW 140lb 4in (HF-C5)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC04Carpet20          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC04Carpet20
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile01             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile01","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile01            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile01
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile02             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile02","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile02            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile02
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile03             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile03","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile03            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile03
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile04             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile04","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile04            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile04
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile05             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile05","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile05            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile05
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile06             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile06","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile06            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile06
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile07             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile07","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile07            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile07
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile08             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile08","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile08            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile08
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile09             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile09","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile09            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile09
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile10             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile10","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile10            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile10
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile11             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile11","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile11            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile11
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile12             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile12","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile12            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile12
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile13             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile13","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile13            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile13
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile14             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile14","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile14            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile14
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile15             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile15","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile15            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile15
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile16             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile16","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile16            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile16
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile17             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile17","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile17            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile17
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile18             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile18","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile18            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile18
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile19             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile19","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile19            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile19
   ..
$LIBRARY-ENTRY Lay_UFictCC06Tile20             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Tile20","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Tile20            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Tile20
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet01           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet01","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet01          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet01
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet02           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet02","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet02          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet02
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet03           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet03","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet03          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet03
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet04           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet04","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet04          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet04
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet05           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet05","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet05          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet05
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet06           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet06","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet06          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet06
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet07           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet07","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet07          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet07
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet08           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet08","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet08          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet08
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet09           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet09","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet09          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet09
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet10           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet10","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet10          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet10
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet11           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet11","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet11          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet11
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet12           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet12","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet12          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet12
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet13           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet13","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet13          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet13
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet14           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet14","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet14          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet14
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet15           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet15","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet15          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet15
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet16           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet16","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet16          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet16
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet17           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet17","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet17          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet17
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet18           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet18","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet18          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet18
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet19           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet19","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet19          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet19
   ..
$LIBRARY-ENTRY Lay_UFictCC06Carpet20           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC06Carpet20","Light Soil, Damp 12in",
      "Conc HW 140lb 6in (HF-C13)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC06Carpet20          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC06Carpet20
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile01             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile01","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile01            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile01
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile02             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile02","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile02            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile02
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile03             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile03","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile03            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile03
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile04             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile04","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile04            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile04
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile05             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile05","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile05            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile05
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile06             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile06","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile06            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile06
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile07             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile07","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile07            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile07
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile08             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile08","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile08            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile08
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile09             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile09","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile09            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile09
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile10             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile10","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile10            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile10
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile11             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile11","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile11            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile11
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile12             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile12","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile12            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile12
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile13             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile13","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile13            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile13
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile14             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile14","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile14            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile14
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile15             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile15","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile15            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile15
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile16             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile16","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile16            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile16
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile17             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile17","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile17            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile17
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile18             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile18","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile18            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile18
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile19             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile19","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile19            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile19
   ..
$LIBRARY-ENTRY Lay_UFictCC12Tile20             LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Tile20","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Linoleum Tile (LT01)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Tile20            CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Tile20
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet01           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet01","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet01          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet01
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet02           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet02","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet02          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet02
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet03           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet03","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet03          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet03
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet04           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet04","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet04          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet04
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet05           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet05","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet05          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet05
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet06           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet06","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet06          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet06
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet07           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet07","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet07          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet07
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet08           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet08","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet08          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet08
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet09           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet09","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet09          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet09
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet10           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet10","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet10          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet10
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet11           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet11","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet11          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet11
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet12           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet12","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet12          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet12
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet13           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet13","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet13          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet13
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet14           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet14","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet14          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet14
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet15           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet15","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet15          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet15
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet16           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet16","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet16          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet16
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet17           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet17","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet17          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet17
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet18           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet18","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet18          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet18
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet19           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet19","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet19          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet19
   ..
$LIBRARY-ENTRY Lay_UFictCC12Carpet20           LAYERS          UFlrCore
$ Description: Interior slab on ground
   INSIDE-FILM-RES = 0.77
   MATERIAL = (
      "Mat_UFictCC12Carpet20","Light Soil, Damp 12in",
      "Conc HW 140lb 12in (HF-C11)","Carpet & Rubber Pad (CP02)")
   ..
$LIBRARY-ENTRY Cons_UFictCC12Carpet20          CONSTRUCTION    UFlrCore
$ Description: Interior slab on ground
   TYPE = LAYERS
   LAYERS = Lay_UFictCC12Carpet20
   ..
