$LIBRARY-ENTRY TwoSpeedFan                     CURVE-FIT       Fan EIR-FPLR
   TYPE = RATIO-FRATIO
   ORDER-OF-FIT = CUBIC              MIN-INPUT-1 = 0.  MAX-INPUT-1 = 1.15
   INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = ( 2.80930E-04, -5.78626E-02,
                    5.86380E-01,  4.71202E-01 )
   ..


$LIBRARY-ENTRY PSZ65to135_ClCap_fT             CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = QUADRATIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 55 MAX-INPUT-1 = 70
   MIN-INPUT-2 = 55 MAX-INPUT-2 = 120   
   COEFFICIENTS = (1.954260E+00, -3.650212E-02, 3.561667E-04,
         6.269644E-03, -4.144196E-05, -5.169714E-05)
      ..
$LIBRARY-ENTRY PSZ65to135_ClSH_fT              CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = QUADRATIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 55 MAX-INPUT-1 = 70
   MIN-INPUT-2 = 55 MAX-INPUT-2 = 120   
   COEFFICIENTS = (2.455665E-01, 9.050745E-02, -1.188833E-03,
         -1.026311E-02, -4.272321E-05, 2.180171E-04)
      ..
$LIBRARY-ENTRY PSZ65to135_EIR_fT               CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = QUADRATIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 55 MAX-INPUT-1 = 70
   MIN-INPUT-2 = 55 MAX-INPUT-2 = 120   
   COEFFICIENTS = (1.302253E-01, 3.699312E-02, -2.778333E-04,
         -2.013198E-02, 2.153973E-04, -6.174286E-05)
      ..
$LIBRARY-ENTRY PSZ65to135_BF_fT                CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = QUADRATIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 55 MAX-INPUT-1 = 70
   MIN-INPUT-2 = 55 MAX-INPUT-2 = 120   
   COEFFICIENTS = (5.703422E+01, -1.770091E+00, 1.445338E-02,
         1.343339E-02, 2.980315E-04, -9.874667E-04)
   MIN-OUTPUT =  0
   MAX-OUTPUT =  3.509
      ..
$LIBRARY-ENTRY PSZ65to135_CEIR_fPLR            CURVE-FIT       CEIR_fPLR
$ Description: Pkg DX EIR_PLR Curve Coefficients
   TYPE = RATIO-FRATIO ORDER-OF-FIT = CUBIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 0 MAX-INPUT-1 = 1.1
   COEFFICIENTS = (1.844000E-02, 1.147620E+00, -2.083300E-01,
         4.227000E-02)
      ..
$LIBRARY-ENTRY PSZ65to135_CLoss_fPLR           CURVE-FIT       CLoss_fPLR
$ Description: C-Loss Curve Coefs for Pkg DX
   TYPE = RATIO-FRATIO ORDER-OF-FIT = CUBIC
   MIN-INPUT-1 = 0 MAX-INPUT-1 = 1.1
   INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.822800E-01, 2.105300E-01, -4.389000E-02,
         9.800000E-03)
   MIN-OUTPUT =  0.8323
   MAX-OUTPUT =  1.1087
      ..
$LIBRARY-ENTRY PSZ65to135_HtCap_fT             CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = QUADRATIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 55 MAX-INPUT-1 = 70
   MIN-INPUT-2 = 55 MAX-INPUT-2 = 120   
   COEFFICIENTS = (0.000000E+00, 0.000000E+00, 0.000000E+00,
         0.000000E+00, 0.000000E+00, 0.000000E+00)
      ..
$LIBRARY-ENTRY PSZ65to135_HIR_fT               CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = QUADRATIC
   INPUT-TYPE = COEFFICIENTS
   MIN-INPUT-1 = 55 MAX-INPUT-1 = 70
   MIN-INPUT-2 = 55 MAX-INPUT-2 = 120   
   COEFFICIENTS = (0.000000E+00, 0.000000E+00, 0.000000E+00,
         0.000000E+00, 0.000000E+00, 0.000000E+00)
      ..
$LIBRARY-ENTRY PSZ65to135_BF_fFlow             CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = RATIO-FT&T  ORDER-OF-FIT     = LINEAR
   INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.000000E+00)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  1
      ..
