$LIBRARY-ENTRY SpltAC1Sp_ClCap_fT              CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.389718E-01, 4.180714E-04, 2.137143E-04,
         8.900324E-03, -2.596259E-05, -1.473000E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp_ClSH_fT               CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (4.677984E+00, -7.371211E-02, 2.893143E-04,
         6.447714E-03, -2.795238E-05, -6.257143E-05)
      ..
$LIBRARY-ENTRY SpltAC1Sp_EIR_fT                CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.275026E-01, -4.615429E-04, 3.960000E-05,
         -6.868805E-03, 2.047959E-04, -1.995429E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp_BF_fT                 CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.554623E+01, -6.592174E-01, 5.116388E-03,
         -2.763760E-02, 3.326322E-04, -5.848495E-04)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.33
      ..
$LIBRARY-ENTRY SpltAC1Sp_CEIR_fPLR_Tem         CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-7.000000E-05, 1.169510E+00, -2.132100E-01,
         4.377000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp_CEIR_fPLR_Mod         CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.200000E-04, 1.201780E+00, -2.614500E-01,
         5.955000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp_CEIR_fPLR_Hot         CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (7.000000E-05, 1.231390E+00, -3.070300E-01,
         7.557000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp_CLoss_fPLR_Tem        CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.518700E-01, 1.700700E-01, -2.194000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp_CLoss_fPLR_Mod        CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.272300E-01, 2.027300E-01, -2.996000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp_CLoss_fPLR_Hot        CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.053000E-01, 2.327000E-01, -3.800000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp_HtCap_fT              CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC1Sp_HIR_fT                CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC1Sp_BF_fFlow              CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
OUTPUT-MIN =  0
OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_ClCap_fT         CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.894492E+00, -3.920125E-02, 4.695299E-04,
         4.068084E-03, -1.335651E-05, -1.008097E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_ClSH_fT          CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.318964E-01, 9.102668E-02, -1.076103E-03,
         -9.654877E-03, -1.689775E-05, 1.466538E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_EIR_fT           CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.419556E+00, 6.563434E-02, -4.469458E-04,
         -2.831027E-03, 1.917192E-04, -2.251254E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_BF_fT            CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.035361E+01, -2.463377E+00, 1.955328E-02,
         9.693401E-02, 2.356870E-04, -2.108063E-03)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.3
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_CEIR_fPLR_Tem    CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.000000E-04, 1.117620E+00, -1.400400E-01,
         2.252000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_CEIR_fPLR_Mod    CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.000000E-05, 1.148140E+00, -1.825200E-01,
         3.430000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_CEIR_fPLR_Hot    CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 1.176280E+00, -2.231000E-01,
         4.682000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_CLoss_fPLR_Tem   CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.934700E-01, 1.177600E-01, -1.123000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_CLoss_fPLR_Mod   CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.687000E-01, 1.485100E-01, -1.721000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_CLoss_fPLR_Hot   CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.466400E-01, 1.768200E-01, -2.346000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_HtCap_fT         CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_HIR_fT           CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC1Sp-lt45_BF_fFlow         CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
OUTPUT-MIN =  0
OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_ClCap_fT         CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.300382E+00, -5.275035E-02, 5.786571E-04,
         5.239770E-03, -1.764177E-05, -1.103318E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_ClSH_fT          CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.005330E+00, 6.087921E-02, -8.766774E-04,
         -1.310949E-02, -1.782982E-05, 1.975622E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_EIR_fT           CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.627910E+00, 8.124672E-02, -5.931791E-04,
         -9.221348E-03, 2.069421E-04, -1.798058E-04)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_BF_fT            CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (5.870876E+01, -1.884684E+00, 1.557167E-02,
         1.588411E-01, 1.507474E-04, -2.794429E-03)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.76
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_CEIR_fPLR_Tem    CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.000000E-04, 1.117620E+00, -1.400400E-01,
         2.252000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_CEIR_fPLR_Mod    CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.000000E-05, 1.148140E+00, -1.825200E-01,
         3.430000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_CEIR_fPLR_Hot    CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 1.176280E+00, -2.231000E-01,
         4.682000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_CLoss_fPLR_Tem   CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.934700E-01, 1.177600E-01, -1.123000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_CLoss_fPLR_Mod   CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.687000E-01, 1.485100E-01, -1.721000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_CLoss_fPLR_Hot   CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.466400E-01, 1.768200E-01, -2.346000E-02)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_HtCap_fT         CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_HIR_fT           CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC1Sp-ge45_BF_fFlow         CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
OUTPUT-MIN =  0
OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_ClCap_fT        CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.446157E+00, -9.133027E-02, 9.239983E-04,
         7.017579E-03, -2.011920E-05, -1.508171E-04)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_ClSH_fT         CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.599409E-01, 7.484282E-02, -9.189473E-04,
         -9.675586E-03, -3.096942E-05, 1.648742E-04)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_EIR_fT          CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-3.022348E+00, 1.345510E-01, -1.003432E-03,
         -1.597843E-02, 2.379210E-04, -1.755615E-04)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_BF_fT           CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (6.689738E+01, -2.013163E+00, 1.588013E-02,
         1.009211E-01, 3.545096E-04, -2.370508E-03)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.92
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_CEIR_fPLR_Tem   CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-7.262500E-03, 1.113365E+00, -1.323450E-01,
         2.624250E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_CEIR_fPLR_Mod   CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.440000E-03, 1.119133E+00, -1.396600E-01,
         2.196750E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_CEIR_fPLR_Hot   CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (6.347500E-03, 1.116228E+00, -1.386200E-01,
         1.604500E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_CLoss_fPLR_Tem  CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.594975E-01, 9.342250E-02, -6.875000E-03)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_CLoss_fPLR_Mod  CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.403200E-01, 1.240650E-01, -1.092750E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_CLoss_fPLR_Hot  CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.229650E-01, 1.525900E-01, -1.561750E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_HtCap_fT        CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_HIR_fT          CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC2SpHiSEER_BF_fFlow        CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.745000E+00, -7.450000E-01)
OUTPUT-MIN =  1
OUTPUT-MAX =  1.189
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_ClCap_fT        CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.490584E+00, -9.134485E-02, 9.565947E-04,
         6.217542E-03, -7.875000E-06, -1.860530E-04)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_ClSH_fT         CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.997067E+00, 1.849693E-03, -3.826839E-04,
         -1.713802E-02, -1.246250E-05, 2.101269E-04)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_EIR_fT          CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-3.457738E+00, 1.551215E-01, -1.143829E-03,
         -2.125080E-02, 2.983857E-04, -2.317138E-04)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_BF_fT           CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.978417E+01, -9.656920E-01, 7.870821E-03,
         2.311484E-01, 1.940798E-04, -3.633244E-03)
OUTPUT-MIN =  0
OUTPUT-MAX =  5.76
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_CEIR_fPLR_Tem   CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.840000E-03, 1.060670E+00, -6.874000E-02,
         5.230000E-03)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_CEIR_fPLR_Mod   CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.460000E-03, 1.103200E+00, -1.193000E-01,
         1.755000E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_CEIR_fPLR_Hot   CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.600000E-04, 1.122400E+00, -1.428200E-01,
         2.058000E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_CLoss_fPLR_Tem  CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.888900E-01, 6.952000E-02, -6.460000E-03)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_CLoss_fPLR_Mod  CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.724300E-01, 9.413000E-02, -7.520000E-03)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_CLoss_fPLR_Hot  CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.562500E-01, 1.211500E-01, -1.241000E-02)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_HtCap_fT        CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_HIR_fT          CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltAC2SpLoSEER_BF_fFlow        CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.745000E+00, -7.450000E-01)
OUTPUT-MIN =  1
OUTPUT-MAX =  1.189
      ..
$LIBRARY-ENTRY SpltHP1SpRes_ClCap_fT           CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.389718E-01, 4.180714E-04, 2.137143E-04,
         8.900324E-03, -2.596259E-05, -1.473000E-04)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_ClSH_fT            CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (4.677984E+00, -7.371211E-02, 2.893143E-04,
         6.447714E-03, -2.795238E-05, -6.257143E-05)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_EIR_fT             CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.275026E-01, -4.615429E-04, 3.960000E-05,
         -6.868805E-03, 2.047959E-04, -1.995429E-04)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_BF_fT              CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.554623E+01, -6.592174E-01, 5.116388E-03,
         -2.763760E-02, 3.326322E-04, -5.848495E-04)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.33
      ..
$LIBRARY-ENTRY SpltHP1SpRes_CEIR_fPLR_Tem      CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-7.000000E-05, 1.169510E+00, -2.132100E-01,
         4.377000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_CEIR_fPLR_Mod      CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.200000E-04, 1.201780E+00, -2.614500E-01,
         5.955000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_CEIR_fPLR_Hot      CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (7.000000E-05, 1.231390E+00, -3.070300E-01,
         7.557000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_CLoss_fPLR_Tem     CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.518700E-01, 1.700700E-01, -2.194000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_CLoss_fPLR_Mod     CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.272300E-01, 2.027300E-01, -2.996000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_CLoss_fPLR_Hot     CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.053000E-01, 2.327000E-01, -3.800000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_HtCap_fT           CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (4.833385E-01, -1.883338E-03, 5.450581E-06,
         1.781500E-02, -1.696476E-06, -6.436783E-05)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_HIR_fT             CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.385744E+00, 5.671749E-03, 5.246975E-05,
         -2.807622E-02, 2.602259E-04, -8.970371E-05)
      ..
$LIBRARY-ENTRY SpltHP1SpRes_BF_fFlow           CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
OUTPUT-MIN =  0
OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY SpltHP2Sp_ClCap_fT              CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.446157E+00, -9.133027E-02, 9.239983E-04,
         7.017579E-03, -2.011920E-05, -1.508171E-04)
      ..
$LIBRARY-ENTRY SpltHP2Sp_ClSH_fT               CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.599409E-01, 7.484282E-02, -9.189473E-04,
         -9.675586E-03, -3.096942E-05, 1.648742E-04)
      ..
$LIBRARY-ENTRY SpltHP2Sp_EIR_fT                CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-3.022348E+00, 1.345510E-01, -1.003432E-03,
         -1.597843E-02, 2.379210E-04, -1.755615E-04)
      ..
$LIBRARY-ENTRY SpltHP2Sp_BF_fT                 CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (6.689738E+01, -2.013163E+00, 1.588013E-02,
         1.009211E-01, 3.545096E-04, -2.370508E-03)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.92
      ..
$LIBRARY-ENTRY SpltHP2Sp_CEIR_fPLR_Tem         CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-7.262500E-03, 1.113365E+00, -1.323450E-01,
         2.624250E-02)
      ..
$LIBRARY-ENTRY SpltHP2Sp_CEIR_fPLR_Mod         CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-1.440000E-03, 1.119133E+00, -1.396600E-01,
         2.196750E-02)
      ..
$LIBRARY-ENTRY SpltHP2Sp_CEIR_fPLR_Hot         CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (6.347500E-03, 1.116228E+00, -1.386200E-01,
         1.604500E-02)
      ..
$LIBRARY-ENTRY SpltHP2Sp_CLoss_fPLR_Tem        CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.594975E-01, 9.342250E-02, -6.875000E-03)
      ..
$LIBRARY-ENTRY SpltHP2Sp_CLoss_fPLR_Mod        CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.403200E-01, 1.240650E-01, -1.092750E-02)
      ..
$LIBRARY-ENTRY SpltHP2Sp_CLoss_fPLR_Hot        CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.229650E-01, 1.525900E-01, -1.561750E-02)
      ..
$LIBRARY-ENTRY SpltHP2Sp_HtCap_fT              CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (4.285056E-01, -9.781311E-04, 5.014184E-15,
         1.530906E-02, 3.901778E-05, -5.038065E-05)
      ..
$LIBRARY-ENTRY SpltHP2Sp_HIR_fT                CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.365961E+00, 3.468768E-03, 6.220870E-05,
         -2.345978E-02, 2.250215E-04, -9.363525E-05)
      ..
$LIBRARY-ENTRY SpltHP2Sp_BF_fFlow              CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.745000E+00, -7.450000E-01)
OUTPUT-MIN =  1
OUTPUT-MAX =  1.189
      ..
$LIBRARY-ENTRY SpltHP1SpCom_ClCap_fT           CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.389718E-01, 4.180714E-04, 2.137143E-04,
         8.900324E-03, -2.596259E-05, -1.473000E-04)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_ClSH_fT            CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (4.677984E+00, -7.371211E-02, 2.893143E-04,
         6.447714E-03, -2.795238E-05, -6.257143E-05)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_EIR_fT             CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.275026E-01, -4.615429E-04, 3.960000E-05,
         -6.868805E-03, 2.047959E-04, -1.995429E-04)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_BF_fT              CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.554623E+01, -6.592174E-01, 5.116388E-03,
         -2.763760E-02, 3.326322E-04, -5.848495E-04)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.33
      ..
$LIBRARY-ENTRY SpltHP1SpCom_CEIR_fPLR_Tem      CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-7.000000E-05, 1.169510E+00, -2.132100E-01,
         4.377000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_CEIR_fPLR_Mod      CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.200000E-04, 1.201780E+00, -2.614500E-01,
         5.955000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_CEIR_fPLR_Hot      CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (7.000000E-05, 1.231390E+00, -3.070300E-01,
         7.557000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_CLoss_fPLR_Tem     CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.518700E-01, 1.700700E-01, -2.194000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_CLoss_fPLR_Mod     CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.272300E-01, 2.027300E-01, -2.996000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_CLoss_fPLR_Hot     CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.053000E-01, 2.327000E-01, -3.800000E-02)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_HtCap_fT           CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (5.325047E-01, -4.995561E-04, -1.912046E-06,
         7.958622E-03, 1.273096E-04, -4.360148E-05)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_HIR_fT             CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.618084E-01, 8.448696E-03, 3.644909E-05,
         -1.018285E-02, 6.860027E-05, -9.263282E-05)
      ..
$LIBRARY-ENTRY SpltHP1SpCom_BF_fFlow           CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
OUTPUT-MIN =  0
OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY SpltACEvap_ClCap_fT             CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (5.026342E-01, 1.344170E-03, 2.132600E-04,
         -8.402200E-04, 6.558000E-05, -1.703100E-04)
      ..
$LIBRARY-ENTRY SpltACEvap_ClSH_fT              CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.726193E+00, 2.210698E-02, -3.947400E-04,
         9.183400E-04, 6.012000E-05, -1.677200E-04)
      ..
$LIBRARY-ENTRY SpltACEvap_EIR_fT               CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.877758E+00, -4.525610E-02, 1.641700E-04,
         1.807855E-02, -1.408800E-04, 1.698700E-04)
      ..
$LIBRARY-ENTRY SpltACEvap_BF_fT                CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (5.667438E+01, -1.665607E+00, 1.245741E-02,
         1.000000E-12, 1.000000E-12, 1.000000E-12)
OUTPUT-MIN =  0
OUTPUT-MAX =  3.97
      ..
$LIBRARY-ENTRY SpltACEvap_CEIR_fPLR_Tem        CURVE-FIT       CEIR_fPLR_Tem
$ Description: Temperate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 1.000000E+00, 0.0,
         0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_CEIR_fPLR_Mod        CURVE-FIT       CEIR_fPLR_Mod
$ Description: Moderate EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 1.000000E+00, 0.0,
         0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_CEIR_fPLR_Hot        CURVE-FIT       CEIR_fPLR_Hot
$ Description: Hot EIR_PLR Curve Fit Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 1.000000E+00, 0.0,
         0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_CLoss_fPLR_Tem       CURVE-FIT       CLoss_fPLR_Tem
$ Description: Temp C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_CLoss_fPLR_Mod       CURVE-FIT       CLoss_fPLR_Mod
$ Description: Mod C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.700000E-01, 3.000000E-02, 0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_CLoss_fPLR_Hot       CURVE-FIT       CLoss_fPLR_Hot
$ Description: Hot C-Loss Curve Fit Coefficients
   TYPE = QUADRATIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.400000E-01, 6.000000E-02, 0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_HtCap_fT             CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_HIR_fT               CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY SpltACEvap_BF_fFlow             CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
OUTPUT-MIN =  0
OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY PSZ65to135_ClCap_fT             CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.954260E+00, -3.650212E-02, 3.561667E-04,
         6.269644E-03, -4.144196E-05, -5.169714E-05)
      ..
$LIBRARY-ENTRY PSZ65to135_ClSH_fT              CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.455665E-01, 9.050745E-02, -1.188833E-03,
         -1.026311E-02, -4.272321E-05, 2.180171E-04)
      ..
$LIBRARY-ENTRY PSZ65to135_EIR_fT               CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.302253E-01, 3.699312E-02, -2.778333E-04,
         -2.013198E-02, 2.153973E-04, -6.174286E-05)
      ..
$LIBRARY-ENTRY PSZ65to135_BF_fT                CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (5.703422E+01, -1.770091E+00, 1.445338E-02,
         1.343339E-02, 2.980315E-04, -9.874667E-04)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  3.509
      ..
$LIBRARY-ENTRY PSZ65to135_CEIR_fPLR            CURVE-FIT       CEIR_fPLR
$ Description: Pkg DX EIR_PLR Curve Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.844000E-02, 1.147620E+00, -2.083300E-01,
         4.227000E-02)
      ..
$LIBRARY-ENTRY PSZ65to135_CLoss_fPLR           CURVE-FIT       CLoss_fPLR
$ Description: C-Loss Curve Coefs for Pkg DX
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.822800E-01, 2.105300E-01, -4.389000E-02,
         9.800000E-03)
   OUTPUT-MIN =  0.8323
   OUTPUT-MAX =  1.1087
      ..
$LIBRARY-ENTRY PSZ65to135_HtCap_fT             CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PSZ65to135_HIR_fT               CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PSZ65to135_BF_fFlow             CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY PSZ135to240_ClCap_fT            CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.504599E+00, -8.081943E-02, 8.026667E-04,
         3.651457E-04, 8.223214E-06, -1.259657E-04)
      ..
$LIBRARY-ENTRY PSZ135to240_ClSH_fT             CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-4.875374E+00, 2.517940E-01, -2.386833E-03,
         -1.772572E-02, -1.275893E-05, 2.386114E-04)
      ..
$LIBRARY-ENTRY PSZ135to240_EIR_fT              CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-2.006738E+00, 8.437850E-02, -6.675000E-04,
         -3.253704E-03, 1.265223E-04, -7.588000E-05)
      ..
$LIBRARY-ENTRY PSZ135to240_BF_fT               CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.721845E+02, -5.522121E+00, 4.580273E-02,
         1.432440E-01, 6.584719E-04, -4.141676E-03)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  4.04
      ..
$LIBRARY-ENTRY PSZ135to240_CEIR_fPLR           CURVE-FIT       CEIR_fPLR
$ Description: Pkg DX EIR_PLR Curve Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.843000E-02, 1.147620E+00, -2.083300E-01,
         4.227000E-02)
      ..
$LIBRARY-ENTRY PSZ135to240_CLoss_fPLR          CURVE-FIT       CLoss_fPLR
$ Description: C-Loss Curve Coefs for Pkg DX
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (8.523600E-01, 2.033300E-01, -4.226000E-02,
         9.380000E-03)
   OUTPUT-MIN =  0.8024
   OUTPUT-MAX =  1.0728
      ..
$LIBRARY-ENTRY PSZ135to240_HtCap_fT            CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PSZ135to240_HIR_fT              CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PSZ135to240_BF_fFlow            CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY PVV240to760_ClCap_fT            CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.477054E+00, -2.873590E-02, 3.802000E-04,
         2.205507E-03, -1.398214E-05, -5.370000E-05)
      ..
$LIBRARY-ENTRY PVV240to760_ClSH_fT             CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.506328E+00, 4.313010E-02, -7.206000E-04,
         -1.265787E-02, -9.982143E-06, 1.777400E-04)
      ..
$LIBRARY-ENTRY PVV240to760_EIR_fT              CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-5.558688E-01, 3.299060E-02, -1.478000E-04,
         5.921640E-03, 1.617500E-04, -3.163200E-04)
      ..
$LIBRARY-ENTRY PVV240to760_BF_fT               CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.656051E+01, -1.355289E+00, 1.082736E-02,
         1.936043E-01, -6.825311E-04, -8.786711E-04)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  3.2
      ..
$LIBRARY-ENTRY PVV240to760_CEIR_fPLR           CURVE-FIT       CEIR_fPLR
$ Description: Pkg DX EIR_PLR Curve Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.241200E-01, 3.762400E-01, 1.293460E+00,
         -7.938200E-01)
      ..
$LIBRARY-ENTRY PVV240to760_CLoss_fPLR          CURVE-FIT       CLoss_fPLR
$ Description: C-Loss Curve Coefs for Pkg DX
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 1.000000E+00, 0.0,
         0.0)
   OUTPUT-MIN =  0.01
   OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY PVV240to760_HtCap_fT            CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PVV240to760_HIR_fT              CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PVV240to760_BF_fFlow            CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  1
      ..
$LIBRARY-ENTRY PSZ240to760_ClCap_fT            CURVE-FIT       ClCap_fT
$ Description: Total Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.245920E+00, -4.590781E-02, 5.164063E-04,
         2.646875E-03, -9.583333E-06, -1.026250E-04)
      ..
$LIBRARY-ENTRY PSZ240to760_ClSH_fT             CURVE-FIT       ClSH_fT
$ Description: Sensible Capacity Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (3.840034E+00, -2.714063E-02, -1.453125E-04,
         -7.646583E-03, -8.916667E-06, 6.875000E-05)
      ..
$LIBRARY-ENTRY PSZ240to760_EIR_fT              CURVE-FIT       EIR_fT
$ Description: EIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (-7.962730E-01, 5.694844E-02, -3.585938E-04,
         -9.886625E-03, 2.090000E-04, -2.131250E-04)
      ..
$LIBRARY-ENTRY PSZ240to760_BF_fT               CURVE-FIT       BF_fT
$ Description: Coil-BF Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (5.813956E+01, -1.738492E+00, 1.269964E-02,
         6.528414E-03, 8.613595E-05, 1.465989E-04)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  3.252
      ..
$LIBRARY-ENTRY PSZ240to760_CEIR_fPLR           CURVE-FIT       CEIR_fPLR
$ Description: Pkg DX EIR_PLR Curve Coefficients
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (2.630580E+00, -9.499990E+00, 1.427181E+01,
         -6.402400E+00)
      ..
$LIBRARY-ENTRY PSZ240to760_CLoss_fPLR          CURVE-FIT       CLoss_fPLR
$ Description: C-Loss Curve Coefs for Pkg DX
   TYPE = CUBIC  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (9.640900E-01, 2.894800E-01, 1.825200E-01,
         -1.311900E-01)
   OUTPUT-MIN =  0.96
   OUTPUT-MAX =  1.3
      ..
$LIBRARY-ENTRY PSZ240to760_HtCap_fT            CURVE-FIT       HtCap_fT
$ Description: Heat pump heating cap curve coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PSZ240to760_HIR_fT              CURVE-FIT       HIR_fT
$ Description: HIR Curve Fit Coefficients
   TYPE = BI-QUADRATIC-T  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (0.0, 0.0, 0.0,
         0.0, 0.0, 0.0)
      ..
$LIBRARY-ENTRY PSZ240to760_BF_fFlow            CURVE-FIT       BF_fFlow
$ Description: BF-FFLOW Curve Coeffients
   TYPE = LINEAR  INPUT-TYPE = COEFFICIENTS
   COEFFICIENTS = (1.000000E+00, 0.0)
   OUTPUT-MIN =  0
   OUTPUT-MAX =  1
      ..
