$LIBRARY-ENTRY CMU MW 12in PolyUFill           MAT             Conc Blk Med Wt 
$Concrete Block, Medium Weight,
$12 Inch, with EPS filled core
 TYPE=PROPERTIES TH=1.00 COND=0.0490 DENS=45.0 S-H=0.2  ..
$LIBRARY-ENTRY CMU MW 6in PolyUFill            MAT             Conc Blk Med Wt 
$Concrete Block, Medium Weight,
$6 Inch, with EPS filled core
 TYPE=PROPERTIES TH=0.50 COND=0.0490 DENS=60.0 S-H=0.2  ..
$LIBRARY-ENTRY CMU MW 8in PolyUFill            MAT             Conc Blk Med Wt 
$Concrete Block, Medium Weight,
$8 Inch, with EPS filled core
 TYPE=PROPERTIES TH=0.6667 COND=.0490 DENS=48.6 S-H=0.2 ..
$LIBRARY-ENTRY Conc LW 30lb 3in                MAT             Concrete 30 lbs 
$Concrete, Light Weight, 30 Lb.,
$3 Inch
 TYPE=PROPERTIES TH=0.25 COND=0.0751 DENS=30.0 S-H=0.2 ..
$LIBRARY-ENTRY MinWool Batt R13                MAT             Batt Insulation 
$Mineral Wool/Fiber, Batt, R-13
 TYPE=PROPERTIES TH=0.2957 COND=0.0210 DENS=0.6 S-H=0.2 ..
$LIBRARY-ENTRY MinWool Batt R21                MAT             Batt Insulation 
$Mineral Wool/Fiber, Batt, R-21
 TYPE=PROPERTIES TH=0.5108 COND=0.0226 DENS=0.6 S-H=0.2 ..
$LIBRARY-ENTRY Carpet & No Pad                 MAT             Carpet          
$Carpet with No Pad
  TYPE=RESISTANCE RES=0.75   ..
$LIBRARY-ENTRY Light Soil, Damp 12in           MAT             Soil            
  TYPE=PROPERTIES  TH=1.0  COND=0.5  DENS=100.0  S-H=0.25  ..
$LIBRARY-ENTRY Polyisocyanurate 1in            MAT             Polyisocyanurate
$Polyisocyanurate, 1 Inch
 TYPE=PROPERTIES TH=0.0833 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polyisocyanurate 1 1/2in        MAT             Polyisocyanurate
$Polyisocyanurate, 1 1/2 Inch
 TYPE=PROPERTIES TH=0.1250 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polyisocyanurate 2in            MAT             Polyisocyanurate
$Polyisocyanurate, 2 Inch
 TYPE=PROPERTIES TH=0.1667 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polyisocyanurate 3in            MAT             Polyisocyanurate
$Polyisocyanurate, 3 Inch
 TYPE=PROPERTIES TH=0.2500 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polyisocyanurate 4in            MAT             Polyisocyanurate
$Polyisocyanurate, 4 Inch
 TYPE=PROPERTIES TH=0.3333 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polyisocyanurate 5in            MAT             Polyisocyanurate
$Polyisocyanurate, 5 Inch
 TYPE=PROPERTIES TH=0.4167 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polyisocyanurate 6in            MAT             Polyisocyanurate
$Polyisocyanurate, 6 Inch
 TYPE=PROPERTIES TH=0.5000 COND=0.0117 DENS=2.0 S-H=0.22  ..
$LIBRARY-ENTRY Polystyrene 1 1/2in             MAT             Polystyrene     
$Polystyrene, Expanded, 1 1/2 Inch
 TYPE=PROPERTIES TH=0.1250 COND=0.0200 DENS=1.8 S-H=0.29  ..
$LIBRARY-ENTRY Polystyrene 4in R-5/in          MAT             Polystyrene     
$Polystyrene, 4 Inch, R-5 per inch
 TYPE=PROPERTIES TH=0.3333 COND=0.0160 DENS=2.5 S-H=0.29  ..
$LIBRARY-ENTRY Polystyrene 5in R-5/in          MAT             Polystyrene     
$Polystyrene, 5 Inch, R-5 per inch
 TYPE=PROPERTIES TH=0.4167 COND=0.0160 DENS=2.5 S-H=0.29  ..
$LIBRARY-ENTRY Polystyrene 6in R-5/in          MAT             Polystyrene     
$Polystyrene, 6 Inch, R-5 per inch
 TYPE=PROPERTIES TH=0.5000 COND=0.0160 DENS=2.5 S-H=0.29  ..
$LIBRARY-ENTRY Polyurethane 1 1/2in            MAT             Polyurethane    
$Polyurethane, Expanded, 1 1/2 Inch
 TYPE=PROPERTIES TH=0.1250 COND=0.0133 DENS=1.5 S-H=0.38 ..
$LIBRARY-ENTRY Polyurethane 5in                MAT             Polyurethane    
$Polyurethane, 5 Inch
 TYPE=PROPERTIES TH=0.4167 COND=0.0133 DENS=1.5 S-H=0.38 ..
$LIBRARY-ENTRY Polyurethane 6in                MAT             Polyurethane    
$Polyurethane, 6 Inch
 TYPE=PROPERTIES TH=0.5000 COND=0.0133 DENS=1.5 S-H=0.38 ..
$LIBRARY-ENTRY 1/4in Spandrel Glass            MAT             Spandrel Glass  
$1/4in Spandrel Glass
 TYPE=PROPERTIES TH=0.0208 COND=0.5900 DENS=172.0 S-H=0.2  ..
