$============================================================================
$==   Constructions   =======================================================
$============================================================================

$LIBRARY-ENTRY Skylt Roof Construction         CONSTRUCTION    Starting Points
   TYPE=U-VALUE U-VALUE=0.001 ABSORPTANCE=0 ROUGHNESS=1 ..

$LIBRARY-ENTRY Default Air Wall Construction   CONSTRUCTION    Starting Points
   TYPE=U-VALUE U-VALUE=2.700 ..

$ Library Entries for Wizard Door Constructions added 10/13/03 - SAC & KJM

$LIBRARY-ENTRY Sgl Lyr Unins Mtl Door          CONSTRUCTION    Doors
TYPE = U-VALUE    U-VALUE = 2.08 ..

$LIBRARY-ENTRY Dbl Lyr Unins Mtl Door          CONSTRUCTION    Doors
TYPE = U-VALUE    U-VALUE = 0.82 ..

$LIBRARY-ENTRY Min 1 3/4 in. Wd Door           CONSTRUCTION    Doors
TYPE = U-VALUE    U-VALUE = 0.56 ..

$LIBRARY-ENTRY Other Wd Door                   CONSTRUCTION    Doors
TYPE = U-VALUE    U-VALUE = 0.69 ..

$ Library Entries to facilitate DEER analysis added 5/16/05 - SAC & KJM
$LIBRARY-ENTRY Mobile Home Door, U = 0.56      CONSTRUCTION    Doors
         TYPE = U-VALUE    U-VALUE = 0.56 ..
$LIBRARY-ENTRY Mobile Home Door, U = 0.53      CONSTRUCTION    Doors
         TYPE = U-VALUE    U-VALUE = 0.53 ..
$LIBRARY-ENTRY Mobile Home Door, U = 0.23      CONSTRUCTION    Doors
         TYPE = U-VALUE    U-VALUE = 0.23 ..

$============================================================================
$==   Circulation Loops   ===================================================
$============================================================================

$LIBRARY-ENTRY DEFAULT-PIPE2                   CIRCULATION-LOOPStarting Points
 TYPE = PIPE2   LOOP-PUMP = DEFAULT-PIPE2-PUMP   ..

$LIBRARY-ENTRY DEFAULT-PIPE2-PUMP              PUMP            Starting Points
 FLOW-RATIO 1.1  HEAD-RATIO 1.1      ..


$============================================================================
$==   HEAT-REJECTION   ======================================================
$============================================================================

$LIBRARY-ENTRY DEFAULT-TWR-PUMP                PUMP            Starting Points
 FLOW-RATIO 1.1  HEAD-RATIO 1.1      ..
$LIBRARY-ENTRY WLHP Tower Pump                 PUMP            Starting Points
 FLOW-RATIO 1.1  HEAD-RATIO 1.1      ..
$LIBRARY-ENTRY DX CW Tower Pump                PUMP            Starting Points
 FLOW-RATIO 1.1  HEAD-RATIO 1.1      ..

$============================================================================
$==   Skylight Shades Schedules   ===========================================
$============================================================================

$LIBRARY-ENTRY Skylight Shades Schedule        SCHEDULE-PD     Misc Schedules
   TYPE=FRACTION
   MONTH=(12) DAY=(31) WEEK-SCHEDULES  =("Skylight Shades Week Sched") ..
$LIBRARY-ENTRY Skylight Shades Week Sched      WEEK-SCHEDULE-PDMisc Schedules
   TYPE=FRACTION
   DAY-SCHEDULES=("Skylight Shades Non-HDD Sched"  &D  &D  &D  &D
                  "Skylight Shades Non-HDD Sched"  &D  &D
                  "Skylight Shades HDD Sched"
                  "Skylight Shades Non-HDD Sched" ) ..
$LIBRARY-ENTRY Skylight Shades Non-HDD Sched   DAY-SCHEDULE-PD Misc Schedules
   TYPE=FRACTION VALUES=(1) ..
$LIBRARY-ENTRY Skylight Shades HDD Sched       DAY-SCHEDULE-PD Misc Schedules
   TYPE=FRACTION VALUES=(0) ..
   
   