$***************************************************************************************************************
$ SECTION START: eQ_Lib_ResHVACAvail.txt
$---------------------------------------------------------------------------------------------------------------
$ DEER2017 Residential Heat Availability Schedules                                                 PRC 4-27-2016
$    - follows T-24 Residential ACM manual 
$---------------------------------------------------------------------------------------------------------------
$  support schedules for Heating and Cooling Availability:
$---------------------------------------------------------------------------------------------------------------
$LIBRARY-ENTRY HVACAvailWeek                   WEEK-SCHEDULE-PDD17 Res HVAC Avail
 TYPE = ON/OFF/TEMP
   DAY-SCHEDULES    =
   ( "HVACAvailDay", &D, &D, &D, &D, &D, &D, &D, &D, &D, &D, &D ) .. 

$LIBRARY-ENTRY HVACNotAvailWeek                WEEK-SCHEDULE-PDD17 Res HVAC Avail
 TYPE = ON/OFF/TEMP
   DAY-SCHEDULES    =
   ( "HVACNotAvailDay", &D, &D, &D, &D, &D, &D, &D, &D, &D, &D, &D ) .. 

$LIBRARY-ENTRY HVACAvailDay                    DAY-SCHEDULE-PD D17 Res HVAC Avail
 TYPE = ON/OFF/TEMP
   VALUES (1) ..
$LIBRARY-ENTRY HVACNotAvailDay                 DAY-SCHEDULE-PD D17 Res HVAC Avail
 TYPE = ON/OFF/TEMP
   VALUES (0) ..


$LIBRARY-ENTRY ResTStatHeat_Day                DAY-SCHEDULE-PD ResTStatHeat
$ Description: Residential heating thermostat set point
   Type = TEMPERATURE
   VALUES = ({ #PA("TStatHtgNit") }, &D, &D, &D, &D, &D,
        { #PA("TStatHtgMrn") }, &D, &D,
        { #PA("TStatHtgDay") }, &D, &D, &D, &D, &D, &D, &D,
        { #PA("TStatHtgEve") }, &D, &D,
        { #PA("TStatHtgNit") }, &D, &D, &D )
$ TStatHtgMrn is the offset, TStatHtgDay is the MAX
$   VALUES = ( {MIN(MAX(65 + #PA("TStatHtgMrn"),55),#PA("TStatHtgDay"))},
$               &D, &D, &D, &D, &D, &D,    
$              {MIN(MAX(68 + #PA("TStatHtgMrn"),55),#PA("TStatHtgDay"))}, 
$               &D, &D, &D, &D, &D, &D, &D, 
$               &D, &D, &D, &D, &D, &D, &D, &D,  
$              {MIN(MAX(65 + #PA("TStatHtgMrn"),55),#PA("TStatHtgDay"))} 
   ..
$LIBRARY-ENTRY HeatNotAvailDay                 DAY-SCHEDULE-PD ResTStatHeat
$ Description: Residential heating thermostat set point when not available
   Type = TEMPERATURE 
   VALUES = (55, &D, &D, &D, &D, &D, &D, &D,
             &D, &D, &D, &D, &D, &D, &D, &D,
             &D, &D, &D, &D, &D, &D, &D, &D) ..
$LIBRARY-ENTRY HeatNotAvailWeek                WEEK-SCHEDULE-PD ResTStatHeat
$ Description: Residential heating thermostat set point
   TYPE = TEMPERATURE
   DAY-SCHEDULES = ("HeatNotAvailDay")  ..

$LIBRARY-ENTRY ResTStatHeat_Wk                 WEEK-SCHEDULE-PD ResTStatHeat
$ Description: Residential heating thermostat set point
   TYPE = TEMPERATURE
   DAY-SCHEDULES = ("ResTStatHeat_Day")  ..


$ TESTING! this schedule reconfigured to be T-24 +- offset
$LIBRARY-ENTRY ResTStatCool_Day                DAY-SCHEDULE-PD ResTStatCool
$ Description: Residential cooling thermostat set point
   Type = TEMPERATURE
   VALUES = ({ #PA("TStatClgNit") }, &D, &D, &D, &D, &D,
        { #PA("TStatClgMrn") }, &D, &D,
        { #PA("TStatClgDay") }, &D, &D, &D, &D, &D, &D, &D,
        { #PA("TStatClgEve") }, &D, &D,
        { #PA("TStatClgNit") }, &D, &D, &D )  
$ TStatClgMrn is the offset, TStatClgDay is the MAX
$   VALUES = ( {MIN(MAX(78 + #PA("TStatClgMrn"),74),#PA("TStatClgDay"))}, 
$              &D, &D, &D, &D, &D, &D,
$              {MIN(MAX(83 + #PA("TStatClgMrn"),74),#PA("TStatClgDay"))},
$               &D, &D, &D, &D, &D,
$              {MIN(MAX(82 + #PA("TStatClgMrn"),74),#PA("TStatClgDay"))}, 
$              {MIN(MAX(81 + #PA("TStatClgMrn"),74),#PA("TStatClgDay"))}, 
$              {MIN(MAX(80 + #PA("TStatClgMrn"),74),#PA("TStatClgDay"))}, 
$              {MIN(MAX(79 + #PA("TStatClgMrn"),74),#PA("TStatClgDay"))}, 
$              {MIN(MAX(78 + #PA("TStatClgMrn"),74),#PA("TStatClgDay")) },
$              &D, &D, &D, &D, &D, &D)
  ..
$LIBRARY-ENTRY ResTStatCool_Wk                 WEEK-SCHEDULE-PD ResTStatCool
$ Description: Residential cooling thermostat set point
   TYPE = TEMPERATURE
   DAY-SCHEDULES = ("ResTStatCool_Day")  ..

$LIBRARY-ENTRY CoolNotAvailDay                 DAY-SCHEDULE-PD ResTStatCool
$ Description: Residential cooling thermostat set point when not available
   Type = TEMPERATURE
   VALUES = (95, &D, &D, &D, &D, &D, &D, &D,
             &D, &D, &D, &D, &D, &D, &D, &D,
             &D, &D, &D, &D, &D, &D, &D, &D) ..
$LIBRARY-ENTRY CoolNotAvailWeek                WEEK-SCHEDULE-PD ResTStatCool
$ Description: Residential cooolin thermostat set point when not available
   TYPE = TEMPERATURE
   DAY-SCHEDULES = ("CoolNotAvailDay")  ..


$---------------------------------------------------------------------------------------------------------------
$  Heat Availability Schedules by Climate Zone
$---------------------------------------------------------------------------------------------------------------
$LIBRARY-ENTRY D_ResTStatHeat_Yr               SCHEDULE-PD     ResTStatHeat
$ Description: Residential heating thermostat set point
   TYPE = TEMPERATURE
   MONTH = ( 12 )
   DAY = ( 31 )
   WEEK-SCHEDULES = ("D_ResTStatHeat_Wk")  ..

$LIBRARY-ENTRY ResHeatTstatCZ01                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE
   MONTH = (12) 
   DAY = (31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk" ) ..

$LIBRARY-ENTRY ResHeatTstatCZ02                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE
   MONTH = (5, 9, 10, 10, 12) 
   DAY = (19, 30, 6, 21, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ03                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 6, 6, 10, 10, 10, 12) 
   DAY = (21, 18, 30, 8, 17, 24, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ04                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (29, 3, 14, 30, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ05                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 5, 5, 6, 6, 6, 7, 8, 8, 8, 9, 9, 9, 10, 10, 10, 12) 
   DAY = (27, 28, 30, 2, 11, 13, 9, 15, 28, 29, 2, 17, 29, 1, 4, 12, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ06                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 11, 11, 11, 12) 
   DAY = (29, 2, 6, 6, 15, 19, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ07                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (2, 2, 4, 5, 5, 11, 12, 12, 12, 12, 12) 
   DAY = (16, 20, 24, 2, 12, 23, 17, 18, 19, 25, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ08                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (3, 3, 4, 4, 4, 11, 11, 11, 12, 12, 12) 
   DAY = (17, 27, 19, 21, 23, 10, 14, 21, 17, 23, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ09                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (3, 3, 4, 5, 5, 11, 11, 11, 12, 12, 12) 
   DAY = (16, 26, 23, 7, 11, 6, 16, 22, 16, 22, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ10                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (3, 3, 4, 5, 5, 11, 12, 12, 12) 
   DAY = (17, 25, 24, 7, 12, 6, 16, 22, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ11                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (27, 4, 14, 29, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ12                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (27, 4, 14, 29, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ13                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 4, 4, 5, 5, 11, 12) 
   DAY = (1, 2, 25, 8, 11, 1, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ14                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (26, 6, 14, 30, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ15                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (1, 1, 2, 2, 2, 2, 3, 4, 4, 11, 12, 12, 12) 
   DAY = (13, 24, 2, 9, 18, 28, 13, 10, 13, 24, 15, 25, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk",
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..
$LIBRARY-ENTRY ResHeatTstatCZ16                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 10, 12) 
   DAY = (23, 1, 31) 
   WEEK-SCHEDULES = ( "ResTStatHeat_Wk", 
                      "HeatNotAvailWeek", "ResTStatHeat_Wk" ) ..


$---------------------------------------------------------------------------------------------------------------
$  Cool Availability Schedules by Climate Zone
$---------------------------------------------------------------------------------------------------------------
$LIBRARY-ENTRY ResCoolTstatCZ01                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (12) 
   DAY = (31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek" ) ..

$LIBRARY-ENTRY ResCoolTstatCZ02                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 9, 10, 10, 12) 
   DAY = (19, 30, 6, 21, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ03                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 6, 6, 10, 10, 10, 12) 
   DAY = (21, 18, 30, 8, 17, 24, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ04                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (29, 3, 14, 30, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ05                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 5, 5, 6, 6, 6, 7, 8, 8, 8, 9, 9, 9, 10, 10, 10, 12) 
   DAY = (27, 28, 30, 2, 11, 13, 9, 15, 28, 29, 2, 17, 29, 1, 4, 12, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ06                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 11, 11, 11, 12) 
   DAY = (29, 2, 6, 6, 15, 19, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ07                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (2, 2, 4, 5, 5, 11, 12, 12, 12, 12, 12) 
   DAY = (16, 20, 24, 2, 12, 23, 17, 18, 19, 25, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ08                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (3, 3, 4, 4, 4, 11, 11, 11, 12, 12, 12) 
   DAY = (17, 27, 19, 21, 23, 10, 14, 21, 17, 23, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ09                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (3, 3, 4, 5, 5, 11, 11, 11, 12, 12, 12) 
   DAY = (16, 26, 23, 7, 11, 6, 16, 22, 16, 22, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ10                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (3, 3, 4, 5, 5, 11, 12, 12, 12) 
   DAY = (17, 25, 24, 7, 12, 6, 16, 22, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ11                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (27, 4, 14, 29, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ12                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (27, 4, 14, 29, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ13                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 4, 4, 5, 5, 11, 12) 
   DAY = (1, 2, 25, 8, 11, 1, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ14                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (4, 5, 5, 10, 12) 
   DAY = (26, 6, 14, 30, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ15                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (1, 1, 2, 2, 2, 2, 3, 4, 4, 11, 12, 12, 12) 
   DAY = (13, 24, 2, 9, 18, 28, 13, 10, 13, 24, 15, 25, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek",
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$LIBRARY-ENTRY ResCoolTstatCZ16                SCHEDULE        D17 Res HVAC Avail
 TYPE = TEMPERATURE   
   MONTH = (5, 10, 12) 
   DAY = (23, 1, 31) 
   WEEK-SCHEDULES = ( "CoolNotAvailWeek", 
                      "ResTStatCool_Wk", "CoolNotAvailWeek" ) ..
$---------------------------------------------------------------------------------------------------------------
$ SECTION END: eQ_Lib_ResHVACAvail.txt
$***************************************************************************************************************
